Furnish and install Anemostat Type 3PD-L, 3PD-F, 3PD-C, 3PD-D, or 3PD-T perforated returns to match perforated supply diffusers. Construction and finish shall be identical to the perforated supply diffusers (without pattern control vanes).