AMSG - Medium Security Grille with Steel Woven mesh Face

Contractor shall furnish and install the mesh security grille, type AMSG as herein specified, where shown on plans. The unit shall be manufactured by Anemostat Products. The mesh security grille shall be all steel construction. The face flange shall be 3/16" steel; the mesh face shall be 10 GA x 1/2" square holes on 5/8" centers steel woven mesh and the sleeve shall be 12 GA steel. The face flange shall be attached to the sleeve with continuous welds. Optional security bars, maximum 6" O.C. shall be welded to the sleeve behind the mesh. The unit shall be secured to the sleeve from the back locking angles and field welded by others. The AMSG unit shall be finished with factory white powder coat.