ASFP/ASFP-RR* - Minimum Security with Lattice Face Plate

Contractor shall furnish and install the security face plate, type ASFP (ASFP-RR), as herein specified or where shown on plans. The unit shall be as manufactured by Anemostat Products. Security face plate type ASFP shall be 12 GA C.R.S.. The face pattern shall be lattice type with 9/16" square holes on 11/16" centers (ASFP-RR 3/16 holes on 9/32" staggered centers). Tamperproof screws shall be provided by the manufacturer for attaching the face plate to a suitable edge. The ASFP shall be finished with factory white powder coat.