FLDL-UL-SG1/FLDL-UL-SG2 - Minimum Security Fire rated Door Louver

Contractor shall furnish and install the security louver, type FLDL-UL-SG1/FLDL-UL-SG2, as herein specified, or where shown on plans. The units shall be as manufactured by Anemostat Products. The FLDL-UL-SG1/FLDL-UL-SG2 fire rated security louver is all steel construction with a face plate of 12 GA with 13/16" square perforations on 1" centers and with louver blades of 18 GA material. The unit shall be furnished with factory white powder coat.