Anemostat Model HU-3 air diffusers shall be furnished and installed where shown on the plans. The diffusers shall consist of three expanding and diverging hollow cones with closed beads with a minimum of three air paths for discharging air from unit heaters in a projection pattern.

The diffuser shall be steel with a baked-on Arctic white finish, or custom color as specified.