RRFP-1/RRFP-2 - Maximum Security perforated face plate(s)

Contractor shall furnish and install risk resistant grille model RRFP-1/RRFP-2 as herein specified or where shown on the plans. The units shall be as manufactured by Anemostat Products. The RRFP-1 and RRFP-2 shall be of all steel welded construction. The face plate will be of 12 GA steel (RRFP-1) with 5/32" on 7/32" perforated holes ( for risk resistance) with a 1/2" "hug tight" lip. A secondary 14 GA face plate mated and spot welded to the front face giving an overall 3/16" seamless face plate appearance (RRFP-2). An optional stainless steel (16-16-mesh) screen will be spot welded to the back of the face plate for further risk and contraband reduction. The face plate will be attached by pinned flat head torx security screws to a suitable edge. Unit shall be finished with factory white powder coat.