Stainless steel linear bar grilles shall be model SSB as manufactured by Anemostat. The grilles shall consist of a (flanged)(straight-sided) outer frame, and core configuration as scheduled.  Core bars shall be (1/8”)(1/4”) wide, fixed on (3/8”)(1/2”) centers, with a (0°)(15°) degree deflection angle. The core assembly shall be welded to the outer frame.  The grille shall be installed using (face screws) (concealed mounting methods).  It shall be the responsibility of the installing contractor to provide appropriate duct supports, angles, and straps to install the grilles as detailed. Grille lengths shall be provided up to 6’ as a single assembly without joints, and up to 18” in height as a 
single core. Longer continuous runs shall be constructed from multiple units, and aligned with alignment hardware from the grille manufacturer.

Grilles shall be constructed from (304)(316) stainless steel and shall be all welded. Floor units shall be constructed with core supports no more than 6” on center.

Where scheduled and as shown, provide mitered corners and (stainless steel)(aluminum)(steel) volume control dampers.

Finish shall be (satin polish)(baked-on white).