SSV432 – MAXIMUM SECURITY ceiling diffuser without faceplate deflection

Contractor shall furnish and install security diffusers, type SSV432 as herein specified, or where shown on plans. The unit shall be provided by Anemostat and will be of all stainless steel assembled and welded construction. The grille shall be made of 16-gauge stainless steel with the outer perimeter (face flange) formed to raise the grille 7/16" from the wall or ceiling. The edge of the face flange shall be manufactured with a beveled slope. The edge shall rest flat on the wall or ceiling.  The cores will be 3-1/4" in depth, comprised of cross sections fabricated with multiple directional changes. The unit shall provide horizontal discharge patterns in single or multiple directions with maximum security without a faceplate. The unit will be mounted with stainless steel tamper proof screws (by others). The SSV432 will have a mill (2B) stainless steel appearance.