SV432 – MAXIMUM SECURITY ceiling diffuser without faceplate deflection

Contractor shall furnish and install security diffusers, type SV432 as herein specified, or where shown on plans. The unit shall be provided by Anemostat and will be of all steel assembled and welded construction. The diffuser shall be made of all 16-gauge steel. The edge of the face flange shall be manufactured with a beveled slope. The edge shall rest flat (± .003”) on the wall or ceiling.  The cores will be 3-1/4” in depth, comprised of cross sections fabricated with multiple directional changes. The unit shall provide horizontal discharge patterns in single or multiple directions with maximum security without a faceplate. The unit will be mounted with stainless steel tamper proof screws (by others). The SV432 will be finished with a beige powder coat (minimum 5 mil. thickness) preceded by a multistage wash and surface preparation process.